## Owning bus names

Using dbus-glib, you typically call RequestName manually to own a name, like in the following excerpt:

    1
    2
    3
    4
    5
    6
    7
    8
    9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    19
    20
    21
    22
    23
    24
    25
    26
    27
    28
    29
    30
    31
    32
    33
    34
    35
    36
    37
    38
    39
    40
    41
    42
    43
    44
    45
    error = NULL;
    res = dbus_g_proxy_call (system_bus_proxy,
                             "RequestName",
                             &error,
                             G_TYPE_STRING, NAME_TO_CLAIM,
                             G_TYPE_UINT,   DBUS_NAME_FLAG_ALLOW_REPLACEMENT,
                             G_TYPE_INVALID,
                             G_TYPE_UINT,   &result,
                             G_TYPE_INVALID);
    if (!res)
      {
        if (error != NULL)
          {
            g_warning ("Failed to acquire %s: %s",
                       NAME_TO_CLAIM, error->message);
            g_error_free (error);
          }
        else
          {
            g_warning ("Failed to acquire %s", NAME_TO_CLAIM);
          }
        goto out;
      }

    if (result != DBUS_REQUEST_NAME_REPLY_PRIMARY_OWNER)
      {
        if (error != NULL)
          {
            g_warning ("Failed to acquire %s: %s",
                       NAME_TO_CLAIM, error->message);
            g_error_free (error);
          }
        else
          {
            g_warning ("Failed to acquire %s", NAME_TO_CLAIM);
          }
        exit (1);
      }

    dbus_g_proxy_add_signal (system_bus_proxy, "NameLost",
                             G_TYPE_STRING, G_TYPE_INVALID);
    dbus_g_proxy_connect_signal (system_bus_proxy, "NameLost",
                                 G_CALLBACK (on_name_lost), NULL, NULL);

    /* further setup ... */

While you can do things this way with GDBus too, using `g_dbus_proxy_call_sync()`, it is much nicer to use the high-level API for this:

    1
    2
    3
    4
    5
    6
    7
    8
    9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    19
    20
    21
    22
    static void
    on_name_acquired (GDBusConnection *connection,
                      const gchar     *name,
                      gpointer         user_data)
    {
      /* further setup ... */
    }

    /* ... */

      owner_id = g_bus_own_name (G_BUS_TYPE_SYSTEM,
                                 NAME_TO_CLAIM,
                                 G_BUS_NAME_OWNER_FLAGS_ALLOW_REPLACEMENT,
                                 on_bus_acquired,
                                 on_name_acquired,
                                 on_name_lost,
                                 NULL,
                                 NULL);

      g_main_loop_run (loop);

      g_bus_unown_name (owner_id);

Note that `g_bus_own_name()` works asynchronously and requires you to enter your mainloop to await the `on_name_aquired()` callback. Also note that in order to avoid race conditions (e.g. when your service is activated by a method call), you have to export your manager object before acquiring the name. The `on_bus_acquired()` callback is the right place to do such preparations.